//===-- X86InstructionInfo.def - X86 Instruction Information ----*- C++ -*-===//
//
// This file describes all of the instructions that the X86 backend uses.  It
// relys on an external 'I' macro being defined that takes the arguments
// specified below, and is used to make all of the information relevant to an
// instruction be in one place.
//
// Note that X86 Instructions always have the destination register listed as
// operand 0, unless it does not produce a value (in which case the TSFlags will
// include X86II::Void).
//
//===----------------------------------------------------------------------===//

// NOTE: No include guards desired

#ifndef I
#errror "Must define I macro before including X86/X86InstructionInfo.def!"
#endif

// Macro to handle the implicit register uses lists...
#ifndef IMPREGSLIST
#define IMPREGSLIST(NAME, ...)
#endif

// Implicit register usage info: O_ is for one register, T_ is for two registers
// NoIR means the instruction does not use implicit registers, in this form.
#define NoIR 0
IMPREGSLIST(O_AL , X86::AL , 0)
IMPREGSLIST(O_AH , X86::AH , 0)
IMPREGSLIST(O_CL , X86::CL , 0)
IMPREGSLIST(O_AX , X86::AX , 0)
IMPREGSLIST(O_DX , X86::DX , 0)
IMPREGSLIST(O_EAX, X86::EAX, 0)
IMPREGSLIST(O_EDX, X86::EDX, 0)
IMPREGSLIST(O_EBP, X86::EBP, 0)
IMPREGSLIST(T_AXDX  , X86::AX , X86::DX , 0)
IMPREGSLIST(T_EAXEDX, X86::EAX, X86::EDX, 0)
IMPREGSLIST(C_CLOBBER, X86::EAX, X86::ECX, X86::EDX,
                       X86::FP0, X86::FP1, X86::FP2, X86::FP3,
                       X86::FP4, X86::FP5, X86::FP6, 0)  // Callee clobber regs

// Floating point registers...
IMPREGSLIST(O_ST0, X86::ST0, 0)
//IMPREGSLIST(O_TOP, X86::TOP, 0)

#undef IMPREGSLIST


// Arguments to be passed into the I macro
//  #1: Enum name - This ends up being the opcode symbol in the X86 namespace
//  #2: Opcode name, as used by the gnu assembler
//  #3: The base opcode for the instruction
//  #4: Instruction Flags - This should be a field or'd together that contains
//      constants from the TargetInstrInfo.h file.
//  #5: Target Specific Flags - Another bitfield containing X86 specific flags
//      that we are interested in for each instruction.  These should be flags
//      defined in X86InstrInfo.h in the X86II namespace.
//  #6: Name of the implicit register uses list
//  #7: Name of the implicit register definitions list
//

// The first instruction must always be the PHI instruction:
I(PHI         , "phi",      0,             0, X86II::Pseudo              , NoIR, NoIR)

// The second instruction must always be the noop instruction:
I(NOOP        , "nop",   0x90,             0, X86II::RawFrm | X86II::Void, NoIR, NoIR)             // nop

// This "instruction" is really an annotation which indicates that a specified
// amount of stack space is needed for an outgoing function call.  This
// instruction is found before any of the stores to the argument slots, which
// use direct ESP references.  If the frame pointer is eliminated, this
// instruction turns into a noop, but if the frame pointer is retained, this
// turns into a 'sub ESP, <amount>'.
//
I(ADJCALLSTACKDOWN, "adjcallstackdown", 0, 0, X86II::Pseudo,               NoIR, NoIR)

// This instruction is used to mark readjustment of the stack after a function
// call.  If the frame pointer is retained, this becomes a 'add ESP, <amount>'
// instruction after the call.
I(ADJCALLSTACKUP  , "adjcallstackup"  , 0, 0, X86II::Pseudo,               NoIR, NoIR)

// This pseudo-instruction is used to record implicit uses of physical registers
// at the end of the function.  This ensures that bad things aren't done to
// registes that are live on exit from the function (for example, EAX).
//
I(IMPLICIT_USE, "implicit_use", 0, 0, X86II::Pseudo, NoIR, NoIR)


// Flow control instructions
I(RET         , "ret",   0xC3,    M_RET_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::Void, NoIR, NoIR)             // ret

I(JMP         , "jmp",   0xE9, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::Void, NoIR, NoIR)             // jmp foo
I(JB          , "jb" ,   0x82, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JAE         , "jae",   0x83, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JE          , "je",    0x84, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // je foo
I(JNE         , "jne",   0x85, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JBE         , "jbe",   0x86, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JA          , "ja" ,   0x87, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JL          , "jl" ,   0x8C, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JGE         , "jge",   0x8D, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JLE         , "jle",   0x8E, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo
I(JG          , "jg" ,   0x8F, M_BRANCH_FLAG | M_TERMINATOR_FLAG, X86II::RawFrm | X86II::TB | X86II::Void, NoIR, NoIR) // jne foo

I(CALLpcrel32 , "call",  0xE8,   M_CALL_FLAG, X86II::Void | X86II::RawFrm, NoIR, C_CLOBBER)        // call pc+42
I(CALLr32     , "call",  0xFF,   M_CALL_FLAG, X86II::Void | X86II::MRMS2r | X86II::Arg32,
                                              NoIR, C_CLOBBER)                                     // call [r32]
I(CALLm32     , "call",  0xFF,   M_CALL_FLAG, X86II::Void | X86II::MRMS2m | X86II::Arg32,
                                              NoIR, C_CLOBBER)                                     // call [m32]

// Misc instructions
I(LEAVE       , "leave", 0xC9,             0, X86II::RawFrm                                 , O_EBP, O_EBP)  // leave
I(BSWAPr32    , "bswap", 0xC8, M_2_ADDR_FLAG, X86II::AddRegFrm  | X86II::Arg32 | X86II::TB    , NoIR, NoIR)  // R32 = bswap R32
I(XCHGrr8     , "xchg" , 0x86,             0, X86II::MRMDestReg | X86II::Arg8                 , NoIR, NoIR)  // xchg(R8, R8)
I(XCHGrr16    , "xchg" , 0x87,             0, X86II::MRMDestReg | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // xchg(R16, R16)
I(XCHGrr32    , "xchg" , 0x87,             0, X86II::MRMDestReg | X86II::Arg32                , NoIR, NoIR)  // xchg(R32, R32)
I(LEAr16      , "lea"  , 0x8D,             0, X86II::MRMSrcMem  | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // R16 = lea [mem]
I(LEAr32      , "lea"  , 0x8D,             0, X86II::MRMSrcMem  | X86II::Arg32                , NoIR, NoIR)  // R32 = lea [mem]


// Move instructions
I(MOVrr8      , "mov",  0x88,             0, X86II::MRMDestReg, NoIR, NoIR)                 // R8  = R8
I(MOVrr16     , "mov",  0x89,             0, X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // R16 = R16
I(MOVrr32     , "mov",  0x89,             0, X86II::MRMDestReg, NoIR, NoIR)                 // R32 = R32
I(MOVir8      , "mov",  0xB0,             0, X86II::AddRegFrm | X86II::Arg8, NoIR, NoIR)                  // R8  = imm8
I(MOVir16     , "mov",  0xB8,             0, X86II::AddRegFrm | X86II::Arg16 | X86II::OpSize, NoIR, NoIR) // R16 = imm16
I(MOVir32     , "mov",  0xB8,             0, X86II::AddRegFrm | X86II::Arg32, NoIR, NoIR)                 // R32 = imm32
I(MOVim8      , "mov",  0xC6,             0, X86II::MRMS0m    | X86II::Arg8, NoIR, NoIR)                  // [mem] = imm8
I(MOVim16     , "mov",  0xC7,             0, X86II::MRMS0m    | X86II::Arg16 | X86II::OpSize, NoIR, NoIR) // [mem] = imm16
I(MOVim32     , "mov",  0xC7,             0, X86II::MRMS0m    | X86II::Arg32, NoIR, NoIR)                 // [mem] = imm32

I(MOVmr8      , "mov",  0x8A,             0, X86II::MRMSrcMem | X86II::Arg8, NoIR, NoIR) // R8  = [mem]
I(MOVmr16     , "mov",  0x8B,             0, X86II::MRMSrcMem | X86II::OpSize |
                                             X86II::Arg16, NoIR, NoIR)                   // R16 = [mem]
I(MOVmr32     , "mov",  0x8B,             0, X86II::MRMSrcMem | X86II::Arg32, NoIR, NoIR)// R32 = [mem]
I(MOVrm8      , "mov",  0x88,             0, X86II::MRMDestMem | X86II::Void |
                                             X86II::Arg8, NoIR, NoIR)                    // [mem] = R8
I(MOVrm16     , "mov",  0x89,             0, X86II::MRMDestMem | X86II::Void |
                                             X86II::OpSize | X86II::Arg16, NoIR, NoIR)   // [mem] = R16
I(MOVrm32     , "mov",  0x89,             0, X86II::MRMDestMem | X86II::Void |
                                             X86II::Arg32, NoIR, NoIR)                   // [mem] = R32

// Arithmetic instructions
I(ADDrr8      , "add",  0x00, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R8  += R8
I(ADDrr16     , "add",  0x01, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // R16 += R16
I(ADDrr32     , "add",  0x01, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::Arg32, NoIR, NoIR)  // R32 += R32

I(ADDri8      , "add",  0x80, M_2_ADDR_FLAG, X86II::MRMS0r     | X86II::Arg8, NoIR, NoIR)  // R8  += imm8
I(ADDri16     , "add",  0x81, M_2_ADDR_FLAG, X86II::MRMS0r     | X86II::OpSize | X86II::Arg16, NoIR, NoIR) // R16 += imm16
I(ADDri32     , "add",  0x81, M_2_ADDR_FLAG, X86II::MRMS0r     | X86II::Arg32, NoIR, NoIR)  // R32 += imm32

I(ADCrr32     , "adc",  0x11, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::Arg32, NoIR, NoIR)  // R32 += R32 + Carry

I(SUBrr8      , "sub",  0x28, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R8  -= R8
I(SUBrr16     , "sub",  0x29, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // R16 -= R16
I(SUBrr32     , "sub",  0x29, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R32 -= R32

I(SUBri8      , "sub",  0x80, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::Arg8 , NoIR, NoIR)      // R8  -= imm8
I(SUBri16     , "sub",  0x81, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::OpSize | X86II::Arg16, NoIR, NoIR)  // R16 -= imm16
I(SUBri32     , "sub",  0x81, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::Arg32, NoIR, NoIR)      // R32 -= imm32

I(SBBrr32     , "sbb",  0x19, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::Arg32, NoIR, NoIR)  // R32 -= R32 + Carry


I(MULr8       , "mul",  0xF6,             0, X86II::MRMS4r | X86II::Void, O_AL, O_AX)       // AX   = AL*R8
I(MULr16      , "mul",  0xF7,             0, X86II::MRMS4r | X86II::Void |                  // DX:AX= AX*R16
                                              X86II::OpSize, O_AX, T_AXDX)
I(MULr32      , "mul",  0xF7,             0, X86II::MRMS4r | X86II::Void, O_EAX, T_EAXEDX)  // ED:EA= EA*R32

// unsigned division/remainder
I(DIVr8       , "div",  0xF6,             0, X86II::MRMS6r | X86II::Void, O_AX, O_AX)       // AX/r8= AL&AH
I(DIVr16      , "div",  0xF7,             0, X86II::MRMS6r | X86II::Void |                  // ED:EA/r16=AX&DX
                                              X86II::OpSize, T_AXDX, T_AXDX)
I(DIVr32      , "div",  0xF7,             0, X86II::MRMS6r | X86II::Void, T_EAXEDX,
                                                                           T_EAXEDX)         // ED:EA/r32=EA&ED

// signed division/remainder
I(IDIVr8      , "idiv", 0xF6,             0, X86II::MRMS7r | X86II::Void, O_AX, O_AX)       // AX/r8= AL&AH
I(IDIVr16     , "idiv", 0xF7,             0, X86II::MRMS7r | X86II::Void |                  // DA/r16=AX&DX
                                              X86II::OpSize, T_AXDX, T_AXDX)
I(IDIVr32     , "idiv", 0xF7,             0, X86II::MRMS7r | X86II::Void, T_EAXEDX,
                                                                           T_EAXEDX)         // DA/r32=EAX&DX

// Logical operators
I(ANDrr8      , "and",   0x20, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R8  &= R8
I(ANDrr16     , "and",   0x21, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // R16 &= R16
I(ANDrr32     , "and",   0x21, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R32 &= R32
I(ANDri8      , "and",   0x80, M_2_ADDR_FLAG, X86II::MRMS4r     | X86II::Arg8 , NoIR, NoIR)  // R8  &= imm8
I(ANDri16     , "and",   0x81, M_2_ADDR_FLAG, X86II::MRMS4r     | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // R16 &= imm16
I(ANDri32     , "and",   0x81, M_2_ADDR_FLAG, X86II::MRMS4r     | X86II::Arg32, NoIR, NoIR)  // R32 &= imm32


I(ORrr8       , "or",    0x08, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R8  |= R8
I(ORrr16      , "or",    0x09, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // R16 |= R16
I(ORrr32      , "or",    0x09, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R32 |= R32
I(ORri8       , "or",    0x80, M_2_ADDR_FLAG, X86II::MRMS1r     | X86II::Arg8 , NoIR, NoIR)  // R8  |= imm8
I(ORri16      , "or",    0x81, M_2_ADDR_FLAG, X86II::MRMS1r     | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // R16 |= imm16
I(ORri32      , "or",    0x81, M_2_ADDR_FLAG, X86II::MRMS1r     | X86II::Arg32, NoIR, NoIR)  // R32 |= imm32

I(XORrr8      , "xor",   0x30, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R8  ^= R8
I(XORrr16     , "xor",   0x31, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // R16 ^= R16
I(XORrr32     , "xor",   0x31, M_2_ADDR_FLAG, X86II::MRMDestReg, NoIR, NoIR)                 // R32 ^= R32
I(XORri8      , "xor",   0x80, M_2_ADDR_FLAG, X86II::MRMS6r     | X86II::Arg8 , NoIR, NoIR)  // R8  ^= imm8
I(XORri16     , "xor",   0x81, M_2_ADDR_FLAG, X86II::MRMS6r     | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // R16 ^= imm16
I(XORri32     , "xor",   0x81, M_2_ADDR_FLAG, X86II::MRMS6r     | X86II::Arg32, NoIR, NoIR)  // R32 ^= imm32

// test instructions are just like and, except they don't generate a result (but
// they do set flags).
I(TESTri8     , "test",  0xF6, 0, X86II::MRMS0r | X86II::Arg8,  NoIR, NoIR)                  // flags = R8 & imm8
I(TESTri16    , "test",  0xF7, 0, X86II::MRMS0r | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // flags = R16 & imm16
I(TESTri32    , "test",  0xF7, 0, X86II::MRMS0r | X86II::Arg32, NoIR, NoIR)                  // flags = R32 & imm32

I(TESTrr8     , "test",  0x84, 0, X86II::MRMDestReg | X86II::Arg8,  NoIR, NoIR)                  // flags = R8 & R8
I(TESTrr16    , "test",  0x85, 0, X86II::MRMDestReg | X86II::Arg16 | X86II::OpSize, NoIR, NoIR)  // flags = R16 & R16
I(TESTrr32    , "test",  0x85, 0, X86II::MRMDestReg | X86II::Arg32, NoIR, NoIR)                  // flags = R32 & R32


// Shift instructions
I(SHLrr8      , "shl",  0xD2, M_2_ADDR_FLAG, X86II::MRMS4r, O_CL, NoIR)                                   // R8   <<= cl
I(SHLrr16     , "shl",  0xD3, M_2_ADDR_FLAG, X86II::MRMS4r | X86II::OpSize, O_CL, NoIR)                   // R16  <<= cl
I(SHLrr32     , "shl",  0xD3, M_2_ADDR_FLAG, X86II::MRMS4r, O_CL, NoIR)                                   // R32  <<= cl
I(SHLir8      , "shl",  0xC0, M_2_ADDR_FLAG, X86II::MRMS4r | X86II::Arg8, NoIR, NoIR)                     // R8   <<= imm8
I(SHLir16     , "shl",  0xC1, M_2_ADDR_FLAG, X86II::MRMS4r | X86II::Arg8 | X86II::OpSize, NoIR, NoIR)     // R16  <<= imm8
I(SHLir32     , "shl",  0xC1, M_2_ADDR_FLAG, X86II::MRMS4r | X86II::Arg8, NoIR, NoIR)                     // R32  <<= imm8
I(SHRrr8      , "shr",  0xD2, M_2_ADDR_FLAG, X86II::MRMS5r, O_CL, NoIR)                                   // R8  >>>= cl
I(SHRrr16     , "shr",  0xD3, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::OpSize, O_CL, NoIR)                   // R16 >>>= cl
I(SHRrr32     , "shr",  0xD3, M_2_ADDR_FLAG, X86II::MRMS5r, O_CL, NoIR)                                   // R32 >>>= cl
I(SHRir8      , "shr",  0xC0, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::Arg8, NoIR, NoIR)                     // R8  >>>= imm8
I(SHRir16     , "shr",  0xC1, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::Arg8 | X86II::OpSize, NoIR, NoIR)     // R16 >>>= imm8
I(SHRir32     , "shr",  0xC1, M_2_ADDR_FLAG, X86II::MRMS5r | X86II::Arg8, NoIR, NoIR)                     // R32 >>>= imm8
I(SARrr8      , "sar",  0xD2, M_2_ADDR_FLAG, X86II::MRMS7r, O_CL, NoIR)                                   // R8   >>= cl
I(SARrr16     , "sar",  0xD3, M_2_ADDR_FLAG, X86II::MRMS7r | X86II::OpSize, O_CL, NoIR)                   // R16  >>= cl
I(SARrr32     , "sar",  0xD3, M_2_ADDR_FLAG, X86II::MRMS7r, O_CL, NoIR)                                   // R32  >>= cl
I(SARir8      , "sar",  0xC0, M_2_ADDR_FLAG, X86II::MRMS7r | X86II::Arg8, NoIR, NoIR)                     // R8   >>= imm8
I(SARir16     , "sar",  0xC1, M_2_ADDR_FLAG, X86II::MRMS7r | X86II::Arg8 | X86II::OpSize, NoIR, NoIR)     // R16  >>= imm8
I(SARir32     , "sar",  0xC1, M_2_ADDR_FLAG, X86II::MRMS7r | X86II::Arg8, NoIR, NoIR)                     // R32  >>= imm8

I(SHLDir32    , "shld",  0xA4, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::TB | X86II::Arg8, NoIR, NoIR)    // R32 >>= R32,R32 imm8
I(SHLDrr32    , "shld",  0xA5, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::TB, O_CL, NoIR)                  // R32 >>= R32,R32 cl
I(SHRDir32    , "shrd",  0xAC, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::TB | X86II::Arg8, NoIR, NoIR)    // R32 >>= R32,R32 imm8
I(SHRDrr32    , "shrd",  0xAD, M_2_ADDR_FLAG, X86II::MRMDestReg | X86II::TB, O_CL, NoIR)                  // R32 >>= R32,R32 cl


// Condition code ops, incl. set if equal/not equal/...
I(SAHF        , "sahf",  0x9E,             0,             X86II::RawFrm, O_AH, NoIR)         // flags = AH
I(SETBr       , "setb",  0x92,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = <  unsign
I(SETAEr      , "setae", 0x93,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = >= unsign
I(SETEr       , "sete",  0x94,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = ==
I(SETNEr      , "setne", 0x95,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = !=
I(SETBEr      , "setbe", 0x96,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = <= unsign
I(SETAr       , "seta",  0x97,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = >  unsign
I(SETLr       , "setl",  0x9C,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = <  signed
I(SETGEr      , "setge", 0x9D,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = >= signed
I(SETLEr      , "setle", 0x9E,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = <= signed
I(SETGr       , "setg",  0x9F,             0, X86II::TB | X86II::MRMS0r, NoIR, NoIR)         // R8 = >  signed

// Conditional moves.  These are modelled as X = cmovXX Y, Z.  Eventually
// register allocated to cmovXX XY, Z
I(CMOVErr16   , "cmove",  0x44, M_2_ADDR_FLAG, X86II::TB | X86II::OpSize | X86II::MRMSrcReg, NoIR, NoIR)    // if ==, R16 = R16
I(CMOVNErr32  , "cmovne", 0x45, M_2_ADDR_FLAG, X86II::TB |                 X86II::MRMSrcReg, NoIR, NoIR)    // if !=, R32 = R32


// Integer comparisons
I(CMPrr8      , "cmpb",  0x38,             0, X86II::Void | X86II::MRMDestReg                , NoIR, NoIR) // compare R8,R8
I(CMPrr16     , "cmpw",  0x39,             0, X86II::Void | X86II::MRMDestReg | X86II::OpSize, NoIR, NoIR) // compare R16,R16
I(CMPrr32     , "cmpl",  0x39,             0, X86II::Void | X86II::MRMDestReg                , NoIR, NoIR) // compare R32,R32
I(CMPri8      , "cmpb",  0x80,             0, X86II::Void | X86II::MRMS7r     | X86II::Arg8  , NoIR, NoIR) // compare R8, imm8
I(CMPri16     , "cmpw",  0x81,             0, X86II::Void | X86II::MRMS7r     | X86II::Arg16 | X86II::OpSize, NoIR, NoIR) // compare R8, imm8
I(CMPri32     , "cmpl",  0x81,             0, X86II::Void | X86II::MRMS7r     | X86II::Arg32 , NoIR, NoIR) // compare R8, imm8

// Sign extenders (first 3 are good for DIV/IDIV; the others are more general)
I(CBW         , "cbw",   0x98,             0, X86II::Void | X86II::RawFrm | X86II::OpSize, O_AL, O_AH)     // AX = signext(AL)
I(CWD         , "cwd",   0x99,             0, X86II::Void | X86II::RawFrm, O_AX, O_DX)                     // DX:AX = signext(AX)
I(CDQ         , "cdq",   0x99,             0, X86II::Void | X86II::RawFrm, O_EAX, O_EDX)                   // EDX:EAX = signext(EAX)
I(MOVSXr16r8  , "movsx", 0xBE,             0, X86II::MRMSrcReg | X86II::TB |                 // R16 = signext(R8)
                                              X86II::OpSize, NoIR, NoIR)
I(MOVSXr32r8  , "movsx", 0xBE,             0, X86II::MRMSrcReg | X86II::TB, NoIR, NoIR)      // R32 = signext(R8)
I(MOVSXr32r16 , "movsx", 0xBF,             0, X86II::MRMSrcReg | X86II::TB, NoIR, NoIR)      // R32 = signext(R16)
I(MOVZXr16r8  , "movzx", 0xB6,             0, X86II::MRMSrcReg | X86II::TB |                 // R16 = zeroext(R8)
                                              X86II::OpSize, NoIR, NoIR)
I(MOVZXr32r8  , "movzx", 0xB6,             0, X86II::MRMSrcReg | X86II::TB, NoIR, NoIR)      // R32 = zeroext(R8)
I(MOVZXr32r16 , "movzx", 0xB7,             0, X86II::MRMSrcReg | X86II::TB, NoIR, NoIR)      // R32 = zeroext(R16)


//===----------------------------------------------------------------------===//
// Floating point support
//===----------------------------------------------------------------------===//

// FIXME: These need to indicate mod/ref sets for FP regs... & FP 'TOP'

// Floating point pseudo instructions...
I(FpMOV       , "FMOV" ,     0, M_PSEUDO_FLAG,                           X86II::ArgF80 | X86II::Pseudo | X86II::SpecialFP, NoIR, NoIR)   // f1 = fmov f2
I(FpADD       , "FADD" ,     0, M_PSEUDO_FLAG,                           X86II::ArgF80 | X86II::Pseudo | X86II::TwoArgFP , NoIR, NoIR)   // f1 = fadd f2, f3
I(FpSUB       , "FSUB" ,     0, M_PSEUDO_FLAG,                           X86II::ArgF80 | X86II::Pseudo | X86II::TwoArgFP , NoIR, NoIR)   // f1 = fsub f2, f3
I(FpMUL       , "FMUL" ,     0, M_PSEUDO_FLAG,                           X86II::ArgF80 | X86II::Pseudo | X86II::TwoArgFP , NoIR, NoIR)   // f1 = fmul f2, f3
I(FpDIV       , "FDIV" ,     0, M_PSEUDO_FLAG,                           X86II::ArgF80 | X86II::Pseudo | X86II::TwoArgFP , NoIR, NoIR)   // f1 = fdiv f2, f3
I(FpUCOM      , "FUCOM",     0, M_PSEUDO_FLAG,             X86II::Void | X86II::ArgF80 | X86II::Pseudo | X86II::TwoArgFP , NoIR, NoIR)   // FPSW = fucom f1, f2

I(FpGETRESULT , "FGETRESULT",0, M_PSEUDO_FLAG,                                           X86II::Pseudo | X86II::SpecialFP, NoIR, NoIR)  // FPR = ST(0)
I(FpSETRESULT , "FSETRESULT",0, M_PSEUDO_FLAG | M_TERMINATOR_FLAG,         X86II::Void | X86II::Pseudo | X86II::SpecialFP, NoIR, NoIR)  // ST(0) = FPR

// Floating point loads & stores...            PREFIX      ARGTYPE         ENCODING        FP INST TYPE      REF   MOD
I(FLDr32      , "fld32",   0xD9,            0,                           X86II::ArgF32 | X86II::MRMS0m | X86II::ZeroArgFP, NoIR, NoIR)   // load float
I(FLDr64      , "fld64",   0xDD,            0,                           X86II::ArgF64 | X86II::MRMS0m | X86II::ZeroArgFP, NoIR, NoIR)   // load double
I(FLDr80      , "fld80",   0xDB,            0,                           X86II::ArgF80 | X86II::MRMS5m | X86II::ZeroArgFP, NoIR, NoIR)   // load extended
I(FLDrr       , "fld"  ,   0xC0,            0, X86II::D9 |               X86II::ArgF80 | X86II::AddRegFrm                , NoIR, NoIR)   // push(ST(i))
I(FILDr16     , "fild16",  0xDF,            0,                           X86II::Arg16  | X86II::MRMS0m | X86II::ZeroArgFP, NoIR, NoIR)   // load signed short
I(FILDr32     , "fild32",  0xDB,            0,                           X86II::Arg32  | X86II::MRMS0m | X86II::ZeroArgFP, NoIR, NoIR)   // load signed int
I(FILDr64     , "fild64",  0xDF,            0,                           X86II::Arg64  | X86II::MRMS5m | X86II::ZeroArgFP, NoIR, NoIR)   // load signed long


I(FSTr32      , "fst32",   0xD9,            0,             X86II::Void | X86II::ArgF32 | X86II::MRMS2m | X86II::OneArgFP , NoIR, NoIR)   // store float
I(FSTr64      , "fst64",   0xDD,            0,             X86II::Void | X86II::ArgF64 | X86II::MRMS2m | X86II::OneArgFP , NoIR, NoIR)   // store double
I(FSTPr32     , "fst32p",  0xD9,            0,             X86II::Void | X86II::ArgF32 | X86II::MRMS3m                   , NoIR, NoIR)   // store float, pop
I(FSTPr64     , "fst64p",  0xDD,            0,             X86II::Void | X86II::ArgF64 | X86II::MRMS3m                   , NoIR, NoIR)   // store double, pop
I(FSTPr80     , "fst80p",  0xDB,            0,             X86II::Void | X86II::ArgF80 | X86II::MRMS7m | X86II::OneArgFP , NoIR, NoIR)   // store extended, pop
I(FSTrr       , "fst"  ,   0xD0,            0, X86II::DD | X86II::Void | X86II::ArgF80 | X86II::AddRegFrm                , NoIR, NoIR)   // ST(i) = ST(0)
I(FSTPrr      , "fstp" ,   0xD8,            0, X86II::DD | X86II::Void | X86II::ArgF80 | X86II::AddRegFrm                , NoIR, NoIR)   // ST(i) = ST(0), pop

I(FISTr16     , "fist16",  0xDF,            0,             X86II::Void | X86II::Arg16  | X86II::MRMS2m | X86II::OneArgFP , NoIR, NoIR)   // store signed short
I(FISTr32     , "fist32",  0xDB,            0,             X86II::Void | X86II::Arg32  | X86II::MRMS2m | X86II::OneArgFP , NoIR, NoIR)   // store signed int
I(FISTPr16    , "fist16p", 0xDF,            0,             X86II::Void | X86II::Arg16  | X86II::MRMS3m                   , NoIR, NoIR)   // store short, pop
I(FISTPr32    , "fist32p", 0xDB,            0,             X86II::Void | X86II::Arg32  | X86II::MRMS3m                   , NoIR, NoIR)   // store int, pop
I(FISTPr64    , "fist64p", 0xDF,            0,             X86II::Void | X86II::Arg64  | X86II::MRMS7m | X86II::OneArgFP , NoIR, NoIR)   // store long, pop


I(FXCH        , "fxch" , 0xC8,              0, X86II::D9 | X86II::Void | X86II::ArgF80 | X86II::AddRegFrm                , O_ST0, O_ST0) // fxch ST(i), ST(0)

// Floating point constant loads...
I(FLD0        , "fld0" , 0xEE,              0, X86II::D9 |               X86II::ArgF80 | X86II::RawFrm | X86II::ZeroArgFP, NoIR, NoIR)   // load +0.0
I(FLD1        , "fld1" , 0xE8,              0, X86II::D9 |               X86II::ArgF80 | X86II::RawFrm | X86II::ZeroArgFP, NoIR, NoIR)   // load +1.0

// Binary arithmetic operations...
I(FADDST0r    , "fadd_0",   0xC0,           0, X86II::D8 |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(0) = ST(0) + ST(i)
I(FADDrST0    , "fadd_i",   0xC0,           0, X86II::DC |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) + ST(0)
I(FADDPrST0   , "faddp_i",  0xC0,           0, X86II::DE |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) + ST(0), pop

I(FSUBRST0r   , "fsubr_0" , 0xE8,           0, X86II::D8 |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(0) = ST(i) - ST(0)
I(FSUBrST0    , "fsub_i"  , 0xE8,           0, X86II::DC |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) - ST(0)
I(FSUBPrST0   , "fsubp_i" , 0xE8,           0, X86II::DE |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) - ST(0), pop

I(FSUBST0r    , "fsub_0"  , 0xE0,           0, X86II::D8 |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(0) = ST(0) - ST(i)
I(FSUBRrST0   , "fsubr_i" , 0xE0,           0, X86II::DC |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(0) - ST(i)
I(FSUBRPrST0  , "fsubrp_i", 0xE0,           0, X86II::DE |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(0) - ST(i), pop

I(FMULST0r    , "fmul_0",   0xC8,           0, X86II::D8 |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(0) = ST(0) * ST(i)
I(FMULrST0    , "fmul_i",   0xC8,           0, X86II::DC |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) * ST(0)
I(FMULPrST0   , "fmulp_i",  0xC8,           0, X86II::DE |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) * ST(0), pop

I(FDIVRST0r   , "fdivr_0" , 0xF8,           0, X86II::D8 |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(0) = ST(i) / ST(0)
I(FDIVrST0    , "fdiv_i"  , 0xF8,           0, X86II::DC |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) / ST(0)
I(FDIVPrST0   , "fdivp_i" , 0xF8,           0, X86II::DE |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(i) / ST(0), pop

I(FDIVST0r    , "fdiv_0"  , 0xF0,           0, X86II::D8 |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(0) = ST(0) / ST(i)
I(FDIVRrST0   , "fdivr_i" , 0xF0,           0, X86II::DC |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(0) / ST(i)
I(FDIVRPrST0  , "fdivrp_i", 0xF0,           0, X86II::DE |               X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // ST(i) = ST(0) / ST(i), pop

// Floating point compares
I(FUCOMr      , "fucom"   , 0xE0,           0, X86II::DD | X86II::Void | X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // FPSW = compare ST(0) with ST(i)
I(FUCOMPr     , "fucomp"  , 0xE8,           0, X86II::DD | X86II::Void | X86II::ArgF80 | X86II::AddRegFrm               , NoIR, NoIR)   // compare, pop
I(FUCOMPPr    , "fucompp" , 0xE9,           0, X86II::DA | X86II::Void                 | X86II::RawFrm                  , NoIR, NoIR)   // compare ST(0) with ST(1), pop, pop

// Floating point flag ops
I(FNSTSWr8    , "fnstsw"  , 0xE0,           0, X86II::DF | X86II::Void                 | X86II::RawFrm                  , NoIR, O_AX)   // AX = fp flags
I(FNSTCWm16   , "fnstcw"  , 0xD9,           0,             X86II::Void | X86II::Arg16  | X86II::MRMS7m                  , NoIR, NoIR)   // [mem16] = X87 Control Word
I(FLDCWm16    , "fldcw"   , 0xD9,           0,             X86II::Void | X86II::Arg16  | X86II::MRMS5m                  , NoIR, NoIR)   // X87 Control Word = [mem16]


// At this point, I is dead, so undefine the macro
#undef I
#undef NoIR

